{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[""]
["Pirkimas: Ksenoniniai šviesos šaltiniai su pakeitimu"]
["TECHNINĖ SPECIFIKACIJA"]
[]
["Nr.","Pavadinimas","Kiekis","Mato vnt.","Tiekėjas nurodo pavadinimą, gamintoją, prekės modelį"]
[]
["1.",""]
["1.1.","Ksenono lempa su pakeitimu",2,"vnt.","Ksenono lempa su pakeitimu,  Olympus, MD-631/MAJ-1817"]
["1.1.1.","Suderinama su Olympus CLV - (S)190 šviesos šaltiniu",null,null,"Suderinama su Olympus CLV - (S)190 šviesos šaltiniu"]
[]
["2.",""]
["2.1.","Ksenono lempa su pakeitimu",2,"vnt."]
["2.1.1.","Komplektuojama su korpusu"]
["2.1.2.","Galia ≥ 300 W"]
["2.1.3.","Suderinama su Conmed šviesos šaltiniais"]