{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":4,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
["Pirkimas: Medžio skiedra (kuras)"]
["TECHNINĖ SPECIFIKACIJA"]
[]
["Nr.","Pavadinimas","Kiekis"]
[]
["1.1.","Biokuras - medžio skiedros","1400","ktm."]
["1.1.1.","Biokuro (skiedrų) kokybė atitinkanti SM1 kodo reikalavimus"]
["1.1.2.","Drėgnumas (min - maks.) 20-45 proc."]
["1.1.3.","Peleningumas - ne daugiau 2 proc."]
["1.1.4.","Frakcijos vidutinis dydis (ilgis-plotis-storis) - 50-50-20 mm (min 80 proc.)"]
["1.1.5.","Frakcijos maksimalus dydis (ilgis-plotis-storis) - 150-60-20 mm (iki 10 proc.)"]
["1.1.6.","Smulkelių frakcijos dydžio dalis biokure ne daugiau 2 proc."]
["1.1.7.","Dominuojanti pirminė žaliava - padžiovinta malkinė mediena, medienos atraižos"]
["1.1.8.","Neleistina žaliava ir priemaišos - chemiškai apdorota mediena (dažyta, lakuota, klijuota) ir kitos aplinkai kenksmingos medžiagos (plastikai, kitos biologinės medžiagos)."]